37 - 1” X 3/8” Bolts

39 - Nuts

4 - Washers

2 - 3” X 3/8” Bolts

34 - ¾” self tapping screws (brown)

5 - ¼” self tapping screws (silver)

4 - End Caps

**6 x 10 – 15 FT. Stand Insulated Blind**

* Raise blind and slide in Legs
* Lower 2” Off Ground
* Install All Braces (Leave Loose)
* Set blind on Level surface
* Pull out on All Legs to Settle The Blind
* Tighten All Bolts
* Raise Platform Install 5- 3/8” Bolts
* Leg #1- 85 ½” Brace to bottom of Platform Leg #2-58” Brace to side of Platform
* Use 6 of the ¾” self tapping screws for the top step extension.

10 Ft Side

88 ½
“

105 ½” ½”½”

43”

85 ½”

128”

160 ½”

3/8 bolt

6 ft side

113 ½”

159”

2

1

4

3

¾” self tapping screws

TOOLS NEEDED

* 9/16” Wrench
* 9/16” Socket and Ratchet
* 3/8 and 5/16 Hex Tips
* Cordless Drill

2

1

4

3

End Caps

**Braces: 1-43”, 1-85 ½”, 2-88 ½”, 2-105 ½”, 4-113 ½”, 4-128 ½“, 4-159”, 2-160 ½“**